{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Macro1","Sheet16"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"Sheet16","index":1,"n_rows":16,"n_cols":10,"rows_kept":16,"merged":[[0,0,0,9],[15,0,24,9]],"flags":["formulas_cached_only"]}
["阿特拉斯办公楼给排水、消防设备材料供货招标"]
["序号","名称","规格型号（mm）","单位","数量","单价","合计","技术要求","用途","备注"]
[1,"室内消火栓消防专用供水泵","流量72，扬程94","台",2,null,null,"按设计要求","消防","参数详见图纸"]
[2,"室外消火栓消防专用供水泵","流量144，扬程32","台",2,null,null,"按设计要求","消防","参数详见图纸"]
[3,"空气压缩机","空气压缩机","台",1,null,null,"按设计要求","消防","参数详见图纸"]
[4,"二氧化氯发生器DEXF-L-100","DEXF-L-100","台",2,null,null,"按设计要求","消防","参数详见图纸"]
[5,"二氧化氯发生器DEXF-L-50","DEXF-L-50","台",1,null,null,"按设计要求","消防","参数详见图纸"]
[6,"喷洒消防专用水泵流量108，扬程90","108，扬程90","台",2,null,null,"按设计要求","消防","参数详见图纸"]
[7,"隔膜式气压水罐","Φ800","台",1,null,null,"按设计要求","消防","参数详见图纸"]
[8,"稳压设备水泵","ZWL-I-X-10","套",1,null,null,"按设计要求","消防","参数详见图纸"]
[9,"无负压供水设备","水泵、无负压罐、控制箱及附件","套",1,null,null,"按设计要求","给排水","参数详见图纸"]
[10,"污水泵","两台一组，带控制箱箱及液位控制器","台",18,null,null,"按设计要求","给排水","参数详见图纸"]
[11,"热水循环泵",null,"台",4,null,null,"按设计要求","给排水","参数详见图纸"]
[12,"太阳能介质循环泵",null,"台",2,null,null,"按设计要求","给排水","参数详见图纸"]
[13,"不锈钢水箱","4*2.5*2.5","台",1,null,null,"按设计要求","给排水","参数详见图纸"]
["本工程不准转包，否则按合同额三分之一罚款。\n本报价包含材料费、装卸费、运输费、利润、税金等综合单价，甲方不再支付任何费用。\n质量要求：1、给排水、消防设备所选用的材料均应满足给排水施工设计总说明内所示指标，所有产品设备均符合国家现行产品标准的规定。2、质保两年。\n技术参数：详见附件给排水图纸技术要求、参数\n付款方式：本工程无预付款，乙方将设备材料运至施工现场由安装单位接收完成付至工程总造价的50%，设备安装调试完成通过检测站及甲方验收，并提交相关工程技术资料后付至95%，一年无质量问题付清，六个月商业承兑付款，开具增值税专用发票。\n售后服务：乙方需安排专人进行设备材料送检，并整理相关工程技术资料，按当地要求完成相关试验，保证通过当地质监部门验收。工程完成后，质保期内设备材料出现质量问题，乙方应在24小时内安排人人员进行免费维修，并承担因此造成的损失。质保期外设备出现质量问题，乙方应积极配合维修，按成本价收取维修费用。\n其他要求：投标单位投标前须提交公司营业执照、资质及安全生产许可等相关资料，交不少于5万元投标保证金,投标单位中标后由董事办将投标保证金的财务收款单连同中标通知书一同转交给基建处，在合同签订后转为安全保证金，工程施工完成无安全事故发生时退还。中标单位须能提供齐全的阿特拉斯开户资料。"]